# S-ON related help

## HTC Gailuak

AdAway-k ez du lan egiten S-ON deituriko gailu bat erabiltzen duzunean. 'ezaugarri' hau HTC gailu askotan aurkitzen da eta AdAway-k hostalari agiria idaztea saihesten du.

## S-ON/S-OFF?

S-OFF esanahi du gailuaren NAND zatia desblokeatuta dagoela eta bertan idatzi daitekeela. HTC gailuen berezko ezarpena S-ON da, honek esanahi du ezin duzula sistemako zenbait eremutara sarbiderik izan ezta errotze egonkor bat bermatu. Gainera, firmware irudien sinadura egiaztapena ere segurtaturik dago S-ON ikurrarekin.

## Nik S-ON edo S-OFF dut?

Boot into the Boot Menu on your device by holding down volume down button while pressing power and the text on top will show the flag status as either S-OFF or S-ON. A full root generally means S-OFF.
More information can be found on www.addictivetips.com. Additional S-OFF methods since Unrevokable (in link) might interest you, namely: Revolutionary, Revone, Firewater, RumRunner, Moonshine, SunShine…

## Konponbidea

Prerequisite: You have to install a working Android SDK with ADB shell on your PC.

1. Boot into the Boot Menu on your device by holding down volume down button while pressing power.
2. Use volume down to select recovery then power to boot it.
3. In clockwork recovery go to "partitions menu".
4. Select mount /system, mount /sdcard and mount /data.
5. Plug in your USB cord and open a command line on your pc.
6. Enter adb shell and type `ln -s /data/hosts /system/etc/hosts` (This creates a symbolic link, which allows AdAway to edit the hosts file stored in `/data` while allowing the OS to use the file as if it were stored in `/system`.)
7. Reboot your device and set Target hosts file to /data/hosts in AdAway's preferences.
8. AdAway-ek lan egin behar du orain.