From: Chris Renshaw <osm0sis@outlook.com>
Date: Fri, 4 Dec 2015 10:35:59 -0400
Subject: [PATCH] ifenslave: add missing headers

Imported from dorimanx's combined ported header toolchain:
https://github.com/dorimanx/android-busybox-ndk
---
 include/linux/ethtool.h    | 940 +++++++++++++++++++++++++++++++++++++++++++++
 include/linux/if_bonding.h | 128 ++++++
 2 files changed, 1068 insertions(+)
 create mode 100644 include/linux/ethtool.h
 create mode 100644 include/linux/if_bonding.h

diff --git a/include/linux/ethtool.h b/include/linux/ethtool.h
new file mode 100644
index 0000000..f96037f
--- /dev/null
+++ b/include/linux/ethtool.h
@@ -0,0 +1,940 @@
+/*
+ * ethtool.h: Defines for Linux ethtool.
+ *
+ * Copyright (C) 1998 David S. Miller (davem@redhat.com)
+ * Copyright 2001 Jeff Garzik <jgarzik@pobox.com>
+ * Portions Copyright 2001 Sun Microsystems (thockin@sun.com)
+ * Portions Copyright 2002 Intel (eli.kupermann@intel.com,
+ *                                christopher.leech@intel.com,
+ *                                scott.feldman@intel.com)
+ * Portions Copyright (C) Sun Microsystems 2008
+ */
+
+#ifndef _LINUX_ETHTOOL_H
+#define _LINUX_ETHTOOL_H
+
+#include <linux/types.h>
+#include <linux/if_ether.h>
+
+/* This should work for both 32 and 64 bit userland. */
+struct ethtool_cmd {
+	__u32	cmd;
+	__u32	supported;	/* Features this interface supports */
+	__u32	advertising;	/* Features this interface advertises */
+	__u16	speed;	        /* The forced speed (lower bits) in
+				 * Mbps. Please use
+				 * ethtool_cmd_speed()/_set() to
+				 * access it */
+	__u8	duplex;		/* Duplex, half or full */
+	__u8	port;		/* Which connector port */
+	__u8	phy_address;
+	__u8	transceiver;	/* Which transceiver to use */
+	__u8	autoneg;	/* Enable or disable autonegotiation */
+	__u8	mdio_support;
+	__u32	maxtxpkt;	/* Tx pkts before generating tx int */
+	__u32	maxrxpkt;	/* Rx pkts before generating rx int */
+	__u16	speed_hi;       /* The forced speed (upper
+				 * bits) in Mbps. Please use
+				 * ethtool_cmd_speed()/_set() to
+				 * access it */
+	__u8	eth_tp_mdix;
+	__u8	reserved2;
+	__u32	lp_advertising;	/* Features the link partner advertises */
+	__u32	reserved[2];
+};
+
+static __inline__ void ethtool_cmd_speed_set(struct ethtool_cmd *ep,
+					 __u32 speed)
+{
+
+	ep->speed = (__u16)speed;
+	ep->speed_hi = (__u16)(speed >> 16);
+}
+
+static __inline__ __u32 ethtool_cmd_speed(const struct ethtool_cmd *ep)
+{
+	return (ep->speed_hi << 16) | ep->speed;
+}
+
+#define ETHTOOL_FWVERS_LEN	32
+#define ETHTOOL_BUSINFO_LEN	32
+/* these strings are set to whatever the driver author decides... */
+struct ethtool_drvinfo {
+	__u32	cmd;
+	char	driver[32];	/* driver short name, "tulip", "eepro100" */
+	char	version[32];	/* driver version string */
+	char	fw_version[ETHTOOL_FWVERS_LEN];	/* firmware version string */
+	char	bus_info[ETHTOOL_BUSINFO_LEN];	/* Bus info for this IF. */
+				/* For PCI devices, use pci_name(pci_dev). */
+	char	reserved1[32];
+	char	reserved2[12];
+				/*
+				 * Some struct members below are filled in
+				 * using ops->get_sset_count().  Obtaining
+				 * this info from ethtool_drvinfo is now
+				 * deprecated; Use ETHTOOL_GSSET_INFO
+				 * instead.
+				 */
+	__u32	n_priv_flags;	/* number of flags valid in ETHTOOL_GPFLAGS */
+	__u32	n_stats;	/* number of u64's from ETHTOOL_GSTATS */
+	__u32	testinfo_len;
+	__u32	eedump_len;	/* Size of data from ETHTOOL_GEEPROM (bytes) */
+	__u32	regdump_len;	/* Size of data from ETHTOOL_GREGS (bytes) */
+};
+
+#define SOPASS_MAX	6
+/* wake-on-lan settings */
+struct ethtool_wolinfo {
+	__u32	cmd;
+	__u32	supported;
+	__u32	wolopts;
+	__u8	sopass[SOPASS_MAX]; /* SecureOn(tm) password */
+};
+
+/* for passing single values */
+struct ethtool_value {
+	__u32	cmd;
+	__u32	data;
+};
+
+/* for passing big chunks of data */
+struct ethtool_regs {
+	__u32	cmd;
+	__u32	version; /* driver-specific, indicates different chips/revs */
+	__u32	len; /* bytes */
+	__u8	data[0];
+};
+
+/* for passing EEPROM chunks */
+struct ethtool_eeprom {
+	__u32	cmd;
+	__u32	magic;
+	__u32	offset; /* in bytes */
+	__u32	len; /* in bytes */
+	__u8	data[0];
+};
+
+/**
+ * struct ethtool_coalesce - coalescing parameters for IRQs and stats updates
+ * @cmd: ETHTOOL_{G,S}COALESCE
+ * @rx_coalesce_usecs: How many usecs to delay an RX interrupt after
+ *	a packet arrives.
+ * @rx_max_coalesced_frames: Maximum number of packets to receive
+ *	before an RX interrupt.
+ * @rx_coalesce_usecs_irq: Same as @rx_coalesce_usecs, except that
+ *	this value applies while an IRQ is being serviced by the host.
+ * @rx_max_coalesced_frames_irq: Same as @rx_max_coalesced_frames,
+ *	except that this value applies while an IRQ is being serviced
+ *	by the host.
+ * @tx_coalesce_usecs: How many usecs to delay a TX interrupt after
+ *	a packet is sent.
+ * @tx_max_coalesced_frames: Maximum number of packets to be sent
+ *	before a TX interrupt.
+ * @tx_coalesce_usecs_irq: Same as @tx_coalesce_usecs, except that
+ *	this value applies while an IRQ is being serviced by the host.
+ * @tx_max_coalesced_frames_irq: Same as @tx_max_coalesced_frames,
+ *	except that this value applies while an IRQ is being serviced
+ *	by the host.
+ * @stats_block_coalesce_usecs: How many usecs to delay in-memory
+ *	statistics block updates.  Some drivers do not have an
+ *	in-memory statistic block, and in such cases this value is
+ *	ignored.  This value must not be zero.
+ * @use_adaptive_rx_coalesce: Enable adaptive RX coalescing.
+ * @use_adaptive_tx_coalesce: Enable adaptive TX coalescing.
+ * @pkt_rate_low: Threshold for low packet rate (packets per second).
+ * @rx_coalesce_usecs_low: How many usecs to delay an RX interrupt after
+ *	a packet arrives, when the packet rate is below @pkt_rate_low.
+ * @rx_max_coalesced_frames_low: Maximum number of packets to be received
+ *	before an RX interrupt, when the packet rate is below @pkt_rate_low.
+ * @tx_coalesce_usecs_low: How many usecs to delay a TX interrupt after
+ *	a packet is sent, when the packet rate is below @pkt_rate_low.
+ * @tx_max_coalesced_frames_low: Maximum nuumber of packets to be sent before
+ *	a TX interrupt, when the packet rate is below @pkt_rate_low.
+ * @pkt_rate_high: Threshold for high packet rate (packets per second).
+ * @rx_coalesce_usecs_high: How many usecs to delay an RX interrupt after
+ *	a packet arrives, when the packet rate is above @pkt_rate_high.
+ * @rx_max_coalesced_frames_high: Maximum number of packets to be received
+ *	before an RX interrupt, when the packet rate is above @pkt_rate_high.
+ * @tx_coalesce_usecs_high: How many usecs to delay a TX interrupt after
+ *	a packet is sent, when the packet rate is above @pkt_rate_high.
+ * @tx_max_coalesced_frames_high: Maximum number of packets to be sent before
+ *	a TX interrupt, when the packet rate is above @pkt_rate_high.
+ * @rate_sample_interval: How often to do adaptive coalescing packet rate
+ *	sampling, measured in seconds.  Must not be zero.
+ *
+ * Each pair of (usecs, max_frames) fields specifies this exit
+ * condition for interrupt coalescing:
+ *	(usecs > 0 && time_since_first_completion >= usecs) ||
+ *	(max_frames > 0 && completed_frames >= max_frames)
+ * It is illegal to set both usecs and max_frames to zero as this
+ * would cause interrupts to never be generated.  To disable
+ * coalescing, set usecs = 0 and max_frames = 1.
+ *
+ * Some implementations ignore the value of max_frames and use the
+ * condition:
+ *	time_since_first_completion >= usecs
+ * This is deprecated.  Drivers for hardware that does not support
+ * counting completions should validate that max_frames == !rx_usecs.
+ *
+ * Adaptive RX/TX coalescing is an algorithm implemented by some
+ * drivers to improve latency under low packet rates and improve
+ * throughput under high packet rates.  Some drivers only implement
+ * one of RX or TX adaptive coalescing.  Anything not implemented by
+ * the driver causes these values to be silently ignored.
+ *
+ * When the packet rate is below @pkt_rate_high but above
+ * @pkt_rate_low (both measured in packets per second) the
+ * normal {rx,tx}_* coalescing parameters are used.
+ */
+struct ethtool_coalesce {
+	__u32	cmd;
+	__u32	rx_coalesce_usecs;
+	__u32	rx_max_coalesced_frames;
+	__u32	rx_coalesce_usecs_irq;
+	__u32	rx_max_coalesced_frames_irq;
+	__u32	tx_coalesce_usecs;
+	__u32	tx_max_coalesced_frames;
+	__u32	tx_coalesce_usecs_irq;
+	__u32	tx_max_coalesced_frames_irq;
+	__u32	stats_block_coalesce_usecs;
+	__u32	use_adaptive_rx_coalesce;
+	__u32	use_adaptive_tx_coalesce;
+	__u32	pkt_rate_low;
+	__u32	rx_coalesce_usecs_low;
+	__u32	rx_max_coalesced_frames_low;
+	__u32	tx_coalesce_usecs_low;
+	__u32	tx_max_coalesced_frames_low;
+	__u32	pkt_rate_high;
+	__u32	rx_coalesce_usecs_high;
+	__u32	rx_max_coalesced_frames_high;
+	__u32	tx_coalesce_usecs_high;
+	__u32	tx_max_coalesced_frames_high;
+	__u32	rate_sample_interval;
+};
+
+/* for configuring RX/TX ring parameters */
+struct ethtool_ringparam {
+	__u32	cmd;	/* ETHTOOL_{G,S}RINGPARAM */
+
+	/* Read only attributes.  These indicate the maximum number
+	 * of pending RX/TX ring entries the driver will allow the
+	 * user to set.
+	 */
+	__u32	rx_max_pending;
+	__u32	rx_mini_max_pending;
+	__u32	rx_jumbo_max_pending;
+	__u32	tx_max_pending;
+
+	/* Values changeable by the user.  The valid values are
+	 * in the range 1 to the "*_max_pending" counterpart above.
+	 */
+	__u32	rx_pending;
+	__u32	rx_mini_pending;
+	__u32	rx_jumbo_pending;
+	__u32	tx_pending;
+};
+
+/**
+ * struct ethtool_channels - configuring number of network channel
+ * @cmd: ETHTOOL_{G,S}CHANNELS
+ * @max_rx: Read only. Maximum number of receive channel the driver support.
+ * @max_tx: Read only. Maximum number of transmit channel the driver support.
+ * @max_other: Read only. Maximum number of other channel the driver support.
+ * @max_combined: Read only. Maximum number of combined channel the driver
+ *	support. Set of queues RX, TX or other.
+ * @rx_count: Valid values are in the range 1 to the max_rx.
+ * @tx_count: Valid values are in the range 1 to the max_tx.
+ * @other_count: Valid values are in the range 1 to the max_other.
+ * @combined_count: Valid values are in the range 1 to the max_combined.
+ *
+ * This can be used to configure RX, TX and other channels.
+ */
+
+struct ethtool_channels {
+	__u32	cmd;
+	__u32	max_rx;
+	__u32	max_tx;
+	__u32	max_other;
+	__u32	max_combined;
+	__u32	rx_count;
+	__u32	tx_count;
+	__u32	other_count;
+	__u32	combined_count;
+};
+
+/* for configuring link flow control parameters */
+struct ethtool_pauseparam {
+	__u32	cmd;	/* ETHTOOL_{G,S}PAUSEPARAM */
+
+	/* If the link is being auto-negotiated (via ethtool_cmd.autoneg
+	 * being true) the user may set 'autoneg' here non-zero to have the
+	 * pause parameters be auto-negotiated too.  In such a case, the
+	 * {rx,tx}_pause values below determine what capabilities are
+	 * advertised.
+	 *
+	 * If 'autoneg' is zero or the link is not being auto-negotiated,
+	 * then {rx,tx}_pause force the driver to use/not-use pause
+	 * flow control.
+	 */
+	__u32	autoneg;
+	__u32	rx_pause;
+	__u32	tx_pause;
+};
+
+#define ETH_GSTRING_LEN		32
+enum ethtool_stringset {
+	ETH_SS_TEST		= 0,
+	ETH_SS_STATS,
+	ETH_SS_PRIV_FLAGS,
+	ETH_SS_NTUPLE_FILTERS,	/* Do not use, GRXNTUPLE is now deprecated */
+	ETH_SS_FEATURES,
+};
+
+/* for passing string sets for data tagging */
+struct ethtool_gstrings {
+	__u32	cmd;		/* ETHTOOL_GSTRINGS */
+	__u32	string_set;	/* string set id e.c. ETH_SS_TEST, etc*/
+	__u32	len;		/* number of strings in the string set */
+	__u8	data[0];
+};
+
+struct ethtool_sset_info {
+	__u32	cmd;		/* ETHTOOL_GSSET_INFO */
+	__u32	reserved;
+	__u64	sset_mask;	/* input: each bit selects an sset to query */
+				/* output: each bit a returned sset */
+	__u32	data[0];	/* ETH_SS_xxx count, in order, based on bits
+				   in sset_mask.  One bit implies one
+				   __u32, two bits implies two
+				   __u32's, etc. */
+};
+
+/**
+ * enum ethtool_test_flags - flags definition of ethtool_test
+ * @ETH_TEST_FL_OFFLINE: if set perform online and offline tests, otherwise
+ *	only online tests.
+ * @ETH_TEST_FL_FAILED: Driver set this flag if test fails.
+ * @ETH_TEST_FL_EXTERNAL_LB: Application request to perform external loopback
+ *	test.
+ * @ETH_TEST_FL_EXTERNAL_LB_DONE: Driver performed the external loopback test
+ */
+
+enum ethtool_test_flags {
+	ETH_TEST_FL_OFFLINE	= (1 << 0),
+	ETH_TEST_FL_FAILED	= (1 << 1),
+	ETH_TEST_FL_EXTERNAL_LB	= (1 << 2),
+	ETH_TEST_FL_EXTERNAL_LB_DONE	= (1 << 3),
+};
+
+/* for requesting NIC test and getting results*/
+struct ethtool_test {
+	__u32	cmd;		/* ETHTOOL_TEST */
+	__u32	flags;		/* ETH_TEST_FL_xxx */
+	__u32	reserved;
+	__u32	len;		/* result length, in number of u64 elements */
+	__u64	data[0];
+};
+
+/* for dumping NIC-specific statistics */
+struct ethtool_stats {
+	__u32	cmd;		/* ETHTOOL_GSTATS */
+	__u32	n_stats;	/* number of u64's being returned */
+	__u64	data[0];
+};
+
+struct ethtool_perm_addr {
+	__u32	cmd;		/* ETHTOOL_GPERMADDR */
+	__u32	size;
+	__u8	data[0];
+};
+
+/* boolean flags controlling per-interface behavior characteristics.
+ * When reading, the flag indicates whether or not a certain behavior
+ * is enabled/present.  When writing, the flag indicates whether
+ * or not the driver should turn on (set) or off (clear) a behavior.
+ *
+ * Some behaviors may read-only (unconditionally absent or present).
+ * If such is the case, return EINVAL in the set-flags operation if the
+ * flag differs from the read-only value.
+ */
+enum ethtool_flags {
+	ETH_FLAG_TXVLAN		= (1 << 7),	/* TX VLAN offload enabled */
+	ETH_FLAG_RXVLAN		= (1 << 8),	/* RX VLAN offload enabled */
+	ETH_FLAG_LRO		= (1 << 15),	/* LRO is enabled */
+	ETH_FLAG_NTUPLE		= (1 << 27),	/* N-tuple filters enabled */
+	ETH_FLAG_RXHASH		= (1 << 28),
+};
+
+/* The following structures are for supporting RX network flow
+ * classification and RX n-tuple configuration. Note, all multibyte
+ * fields, e.g., ip4src, ip4dst, psrc, pdst, spi, etc. are expected to
+ * be in network byte order.
+ */
+
+/**
+ * struct ethtool_tcpip4_spec - flow specification for TCP/IPv4 etc.
+ * @ip4src: Source host
+ * @ip4dst: Destination host
+ * @psrc: Source port
+ * @pdst: Destination port
+ * @tos: Type-of-service
+ *
+ * This can be used to specify a TCP/IPv4, UDP/IPv4 or SCTP/IPv4 flow.
+ */
+struct ethtool_tcpip4_spec {
+	__be32	ip4src;
+	__be32	ip4dst;
+	__be16	psrc;
+	__be16	pdst;
+	__u8    tos;
+};
+
+/**
+ * struct ethtool_ah_espip4_spec - flow specification for IPsec/IPv4
+ * @ip4src: Source host
+ * @ip4dst: Destination host
+ * @spi: Security parameters index
+ * @tos: Type-of-service
+ *
+ * This can be used to specify an IPsec transport or tunnel over IPv4.
+ */
+struct ethtool_ah_espip4_spec {
+	__be32	ip4src;
+	__be32	ip4dst;
+	__be32	spi;
+	__u8    tos;
+};
+
+#define	ETH_RX_NFC_IP4	1
+
+/**
+ * struct ethtool_usrip4_spec - general flow specification for IPv4
+ * @ip4src: Source host
+ * @ip4dst: Destination host
+ * @l4_4_bytes: First 4 bytes of transport (layer 4) header
+ * @tos: Type-of-service
+ * @ip_ver: Value must be %ETH_RX_NFC_IP4; mask must be 0
+ * @proto: Transport protocol number; mask must be 0
+ */
+struct ethtool_usrip4_spec {
+	__be32	ip4src;
+	__be32	ip4dst;
+	__be32	l4_4_bytes;
+	__u8    tos;
+	__u8    ip_ver;
+	__u8    proto;
+};
+
+union ethtool_flow_union {
+	struct ethtool_tcpip4_spec		tcp_ip4_spec;
+	struct ethtool_tcpip4_spec		udp_ip4_spec;
+	struct ethtool_tcpip4_spec		sctp_ip4_spec;
+	struct ethtool_ah_espip4_spec		ah_ip4_spec;
+	struct ethtool_ah_espip4_spec		esp_ip4_spec;
+	struct ethtool_usrip4_spec		usr_ip4_spec;
+	struct ethhdr				ether_spec;
+	__u8					hdata[60];
+};
+
+struct ethtool_flow_ext {
+	__be16	vlan_etype;
+	__be16	vlan_tci;
+	__be32	data[2];
+};
+
+/**
+ * struct ethtool_rx_flow_spec - classification rule for RX flows
+ * @flow_type: Type of match to perform, e.g. %TCP_V4_FLOW
+ * @h_u: Flow fields to match (dependent on @flow_type)
+ * @h_ext: Additional fields to match
+ * @m_u: Masks for flow field bits to be matched
+ * @m_ext: Masks for additional field bits to be matched
+ *	Note, all additional fields must be ignored unless @flow_type
+ *	includes the %FLOW_EXT flag.
+ * @ring_cookie: RX ring/queue index to deliver to, or %RX_CLS_FLOW_DISC
+ *	if packets should be discarded
+ * @location: Location of rule in the table.  Locations must be
+ *	numbered such that a flow matching multiple rules will be
+ *	classified according to the first (lowest numbered) rule.
+ */
+struct ethtool_rx_flow_spec {
+	__u32		flow_type;
+	union ethtool_flow_union h_u;
+	struct ethtool_flow_ext h_ext;
+	union ethtool_flow_union m_u;
+	struct ethtool_flow_ext m_ext;
+	__u64		ring_cookie;
+	__u32		location;
+};
+
+/**
+ * struct ethtool_rxnfc - command to get or set RX flow classification rules
+ * @cmd: Specific command number - %ETHTOOL_GRXFH, %ETHTOOL_SRXFH,
+ *	%ETHTOOL_GRXRINGS, %ETHTOOL_GRXCLSRLCNT, %ETHTOOL_GRXCLSRULE,
+ *	%ETHTOOL_GRXCLSRLALL, %ETHTOOL_SRXCLSRLDEL or %ETHTOOL_SRXCLSRLINS
+ * @flow_type: Type of flow to be affected, e.g. %TCP_V4_FLOW
+ * @data: Command-dependent value
+ * @fs: Flow classification rule
+ * @rule_cnt: Number of rules to be affected
+ * @rule_locs: Array of used rule locations
+ *
+ * For %ETHTOOL_GRXFH and %ETHTOOL_SRXFH, @data is a bitmask indicating
+ * the fields included in the flow hash, e.g. %RXH_IP_SRC.  The following
+ * structure fields must not be used.
+ *
+ * For %ETHTOOL_GRXRINGS, @data is set to the number of RX rings/queues
+ * on return.
+ *
+ * For %ETHTOOL_GRXCLSRLCNT, @rule_cnt is set to the number of defined
+ * rules on return.
+ *
+ * For %ETHTOOL_GRXCLSRULE, @fs.@location specifies the location of an
+ * existing rule on entry and @fs contains the rule on return.
+ *
+ * For %ETHTOOL_GRXCLSRLALL, @rule_cnt specifies the array size of the
+ * user buffer for @rule_locs on entry.  On return, @data is the size
+ * of the rule table, @rule_cnt is the number of defined rules, and
+ * @rule_locs contains the locations of the defined rules.  Drivers
+ * must use the second parameter to get_rxnfc() instead of @rule_locs.
+ *
+ * For %ETHTOOL_SRXCLSRLINS, @fs specifies the rule to add or update.
+ * @fs.@location specifies the location to use and must not be ignored.
+ *
+ * For %ETHTOOL_SRXCLSRLDEL, @fs.@location specifies the location of an
+ * existing rule on entry.
+ */
+struct ethtool_rxnfc {
+	__u32				cmd;
+	__u32				flow_type;
+	__u64				data;
+	struct ethtool_rx_flow_spec	fs;
+	__u32				rule_cnt;
+	__u32				rule_locs[0];
+};
+
+
+/**
+ * struct ethtool_rxfh_indir - command to get or set RX flow hash indirection
+ * @cmd: Specific command number - %ETHTOOL_GRXFHINDIR or %ETHTOOL_SRXFHINDIR
+ * @size: On entry, the array size of the user buffer.  On return from
+ *	%ETHTOOL_GRXFHINDIR, the array size of the hardware indirection table.
+ * @ring_index: RX ring/queue index for each hash value
+ */
+struct ethtool_rxfh_indir {
+	__u32	cmd;
+	__u32	size;
+	__u32	ring_index[0];
+};
+
+/**
+ * struct ethtool_rx_ntuple_flow_spec - specification for RX flow filter
+ * @flow_type: Type of match to perform, e.g. %TCP_V4_FLOW
+ * @h_u: Flow field values to match (dependent on @flow_type)
+ * @m_u: Masks for flow field value bits to be ignored
+ * @vlan_tag: VLAN tag to match
+ * @vlan_tag_mask: Mask for VLAN tag bits to be ignored
+ * @data: Driver-dependent data to match
+ * @data_mask: Mask for driver-dependent data bits to be ignored
+ * @action: RX ring/queue index to deliver to (non-negative) or other action
+ *	(negative, e.g. %ETHTOOL_RXNTUPLE_ACTION_DROP)
+ *
+ * For flow types %TCP_V4_FLOW, %UDP_V4_FLOW and %SCTP_V4_FLOW, where
+ * a field value and mask are both zero this is treated as if all mask
+ * bits are set i.e. the field is ignored.
+ */
+struct ethtool_rx_ntuple_flow_spec {
+	__u32		 flow_type;
+	union {
+		struct ethtool_tcpip4_spec		tcp_ip4_spec;
+		struct ethtool_tcpip4_spec		udp_ip4_spec;
+		struct ethtool_tcpip4_spec		sctp_ip4_spec;
+		struct ethtool_ah_espip4_spec		ah_ip4_spec;
+		struct ethtool_ah_espip4_spec		esp_ip4_spec;
+		struct ethtool_usrip4_spec		usr_ip4_spec;
+		struct ethhdr				ether_spec;
+		__u8					hdata[72];
+	} h_u, m_u;
+
+	__u16	        vlan_tag;
+	__u16	        vlan_tag_mask;
+	__u64		data;
+	__u64		data_mask;
+
+	__s32		action;
+#define ETHTOOL_RXNTUPLE_ACTION_DROP	(-1)	/* drop packet */
+#define ETHTOOL_RXNTUPLE_ACTION_CLEAR	(-2)	/* clear filter */
+};
+
+/**
+ * struct ethtool_rx_ntuple - command to set or clear RX flow filter
+ * @cmd: Command number - %ETHTOOL_SRXNTUPLE
+ * @fs: Flow filter specification
+ */
+struct ethtool_rx_ntuple {
+	__u32					cmd;
+	struct ethtool_rx_ntuple_flow_spec	fs;
+};
+
+#define ETHTOOL_FLASH_MAX_FILENAME	128
+enum ethtool_flash_op_type {
+	ETHTOOL_FLASH_ALL_REGIONS	= 0,
+};
+
+/* for passing firmware flashing related parameters */
+struct ethtool_flash {
+	__u32	cmd;
+	__u32	region;
+	char	data[ETHTOOL_FLASH_MAX_FILENAME];
+};
+
+/**
+ * struct ethtool_dump - used for retrieving, setting device dump
+ * @cmd: Command number - %ETHTOOL_GET_DUMP_FLAG, %ETHTOOL_GET_DUMP_DATA, or
+ * 	%ETHTOOL_SET_DUMP
+ * @version: FW version of the dump, filled in by driver
+ * @flag: driver dependent flag for dump setting, filled in by driver during
+ * 	  get and filled in by ethtool for set operation
+ * @len: length of dump data, used as the length of the user buffer on entry to
+ * 	 %ETHTOOL_GET_DUMP_DATA and this is returned as dump length by driver
+ * 	 for %ETHTOOL_GET_DUMP_FLAG command
+ * @data: data collected for get dump data operation
+ */
+struct ethtool_dump {
+	__u32	cmd;
+	__u32	version;
+	__u32	flag;
+	__u32	len;
+	__u8	data[0];
+};
+
+/* for returning and changing feature sets */
+
+/**
+ * struct ethtool_get_features_block - block with state of 32 features
+ * @available: mask of changeable features
+ * @requested: mask of features requested to be enabled if possible
+ * @active: mask of currently enabled features
+ * @never_changed: mask of features not changeable for any device
+ */
+struct ethtool_get_features_block {
+	__u32	available;
+	__u32	requested;
+	__u32	active;
+	__u32	never_changed;
+};
+
+/**
+ * struct ethtool_gfeatures - command to get state of device's features
+ * @cmd: command number = %ETHTOOL_GFEATURES
+ * @size: in: number of elements in the features[] array;
+ *       out: number of elements in features[] needed to hold all features
+ * @features: state of features
+ */
+struct ethtool_gfeatures {
+	__u32	cmd;
+	__u32	size;
+	struct ethtool_get_features_block features[0];
+};
+
+/**
+ * struct ethtool_set_features_block - block with request for 32 features
+ * @valid: mask of features to be changed
+ * @requested: values of features to be changed
+ */
+struct ethtool_set_features_block {
+	__u32	valid;
+	__u32	requested;
+};
+
+/**
+ * struct ethtool_sfeatures - command to request change in device's features
+ * @cmd: command number = %ETHTOOL_SFEATURES
+ * @size: array size of the features[] array
+ * @features: feature change masks
+ */
+struct ethtool_sfeatures {
+	__u32	cmd;
+	__u32	size;
+	struct ethtool_set_features_block features[0];
+};
+
+/*
+ * %ETHTOOL_SFEATURES changes features present in features[].valid to the
+ * values of corresponding bits in features[].requested. Bits in .requested
+ * not set in .valid or not changeable are ignored.
+ *
+ * Returns %EINVAL when .valid contains undefined or never-changeable bits
+ * or size is not equal to required number of features words (32-bit blocks).
+ * Returns >= 0 if request was completed; bits set in the value mean:
+ *   %ETHTOOL_F_UNSUPPORTED - there were bits set in .valid that are not
+ *	changeable (not present in %ETHTOOL_GFEATURES' features[].available)
+ *	those bits were ignored.
+ *   %ETHTOOL_F_WISH - some or all changes requested were recorded but the
+ *      resulting state of bits masked by .valid is not equal to .requested.
+ *      Probably there are other device-specific constraints on some features
+ *      in the set. When %ETHTOOL_F_UNSUPPORTED is set, .valid is considered
+ *      here as though ignored bits were cleared.
+ *   %ETHTOOL_F_COMPAT - some or all changes requested were made by calling
+ *      compatibility functions. Requested offload state cannot be properly
+ *      managed by kernel.
+ *
+ * Meaning of bits in the masks are obtained by %ETHTOOL_GSSET_INFO (number of
+ * bits in the arrays - always multiple of 32) and %ETHTOOL_GSTRINGS commands
+ * for ETH_SS_FEATURES string set. First entry in the table corresponds to least
+ * significant bit in features[0] fields. Empty strings mark undefined features.
+ */
+enum ethtool_sfeatures_retval_bits {
+	ETHTOOL_F_UNSUPPORTED__BIT,
+	ETHTOOL_F_WISH__BIT,
+	ETHTOOL_F_COMPAT__BIT,
+};
+
+#define ETHTOOL_F_UNSUPPORTED   (1 << ETHTOOL_F_UNSUPPORTED__BIT)
+#define ETHTOOL_F_WISH          (1 << ETHTOOL_F_WISH__BIT)
+#define ETHTOOL_F_COMPAT        (1 << ETHTOOL_F_COMPAT__BIT)
+
+
+/* CMDs currently supported */
+#define ETHTOOL_GSET		0x00000001 /* Get settings. */
+#define ETHTOOL_SSET		0x00000002 /* Set settings. */
+#define ETHTOOL_GDRVINFO	0x00000003 /* Get driver info. */
+#define ETHTOOL_GREGS		0x00000004 /* Get NIC registers. */
+#define ETHTOOL_GWOL		0x00000005 /* Get wake-on-lan options. */
+#define ETHTOOL_SWOL		0x00000006 /* Set wake-on-lan options. */
+#define ETHTOOL_GMSGLVL		0x00000007 /* Get driver message level */
+#define ETHTOOL_SMSGLVL		0x00000008 /* Set driver msg level. */
+#define ETHTOOL_NWAY_RST	0x00000009 /* Restart autonegotiation. */
+/* Get link status for host, i.e. whether the interface *and* the
+ * physical port (if there is one) are up (ethtool_value). */
+#define ETHTOOL_GLINK		0x0000000a
+#define ETHTOOL_GEEPROM		0x0000000b /* Get EEPROM data */
+#define ETHTOOL_SEEPROM		0x0000000c /* Set EEPROM data. */
+#define ETHTOOL_GCOALESCE	0x0000000e /* Get coalesce config */
+#define ETHTOOL_SCOALESCE	0x0000000f /* Set coalesce config. */
+#define ETHTOOL_GRINGPARAM	0x00000010 /* Get ring parameters */
+#define ETHTOOL_SRINGPARAM	0x00000011 /* Set ring parameters. */
+#define ETHTOOL_GPAUSEPARAM	0x00000012 /* Get pause parameters */
+#define ETHTOOL_SPAUSEPARAM	0x00000013 /* Set pause parameters. */
+#define ETHTOOL_GRXCSUM		0x00000014 /* Get RX hw csum enable (ethtool_value) */
+#define ETHTOOL_SRXCSUM		0x00000015 /* Set RX hw csum enable (ethtool_value) */
+#define ETHTOOL_GTXCSUM		0x00000016 /* Get TX hw csum enable (ethtool_value) */
+#define ETHTOOL_STXCSUM		0x00000017 /* Set TX hw csum enable (ethtool_value) */
+#define ETHTOOL_GSG		0x00000018 /* Get scatter-gather enable
+					    * (ethtool_value) */
+#define ETHTOOL_SSG		0x00000019 /* Set scatter-gather enable
+					    * (ethtool_value). */
+#define ETHTOOL_TEST		0x0000001a /* execute NIC self-test. */
+#define ETHTOOL_GSTRINGS	0x0000001b /* get specified string set */
+#define ETHTOOL_PHYS_ID		0x0000001c /* identify the NIC */
+#define ETHTOOL_GSTATS		0x0000001d /* get NIC-specific statistics */
+#define ETHTOOL_GTSO		0x0000001e /* Get TSO enable (ethtool_value) */
+#define ETHTOOL_STSO		0x0000001f /* Set TSO enable (ethtool_value) */
+#define ETHTOOL_GPERMADDR	0x00000020 /* Get permanent hardware address */
+#define ETHTOOL_GUFO		0x00000021 /* Get UFO enable (ethtool_value) */
+#define ETHTOOL_SUFO		0x00000022 /* Set UFO enable (ethtool_value) */
+#define ETHTOOL_GGSO		0x00000023 /* Get GSO enable (ethtool_value) */
+#define ETHTOOL_SGSO		0x00000024 /* Set GSO enable (ethtool_value) */
+#define ETHTOOL_GFLAGS		0x00000025 /* Get flags bitmap(ethtool_value) */
+#define ETHTOOL_SFLAGS		0x00000026 /* Set flags bitmap(ethtool_value) */
+#define ETHTOOL_GPFLAGS		0x00000027 /* Get driver-private flags bitmap */
+#define ETHTOOL_SPFLAGS		0x00000028 /* Set driver-private flags bitmap */
+
+#define ETHTOOL_GRXFH		0x00000029 /* Get RX flow hash configuration */
+#define ETHTOOL_SRXFH		0x0000002a /* Set RX flow hash configuration */
+#define ETHTOOL_GGRO		0x0000002b /* Get GRO enable (ethtool_value) */
+#define ETHTOOL_SGRO		0x0000002c /* Set GRO enable (ethtool_value) */
+#define ETHTOOL_GRXRINGS	0x0000002d /* Get RX rings available for LB */
+#define ETHTOOL_GRXCLSRLCNT	0x0000002e /* Get RX class rule count */
+#define ETHTOOL_GRXCLSRULE	0x0000002f /* Get RX classification rule */
+#define ETHTOOL_GRXCLSRLALL	0x00000030 /* Get all RX classification rule */
+#define ETHTOOL_SRXCLSRLDEL	0x00000031 /* Delete RX classification rule */
+#define ETHTOOL_SRXCLSRLINS	0x00000032 /* Insert RX classification rule */
+#define ETHTOOL_FLASHDEV	0x00000033 /* Flash firmware to device */
+#define ETHTOOL_RESET		0x00000034 /* Reset hardware */
+#define ETHTOOL_SRXNTUPLE	0x00000035 /* Add an n-tuple filter to device */
+#define ETHTOOL_GRXNTUPLE	0x00000036 /* deprecated */
+#define ETHTOOL_GSSET_INFO	0x00000037 /* Get string set info */
+#define ETHTOOL_GRXFHINDIR	0x00000038 /* Get RX flow hash indir'n table */
+#define ETHTOOL_SRXFHINDIR	0x00000039 /* Set RX flow hash indir'n table */
+
+#define ETHTOOL_GFEATURES	0x0000003a /* Get device offload settings */
+#define ETHTOOL_SFEATURES	0x0000003b /* Change device offload settings */
+#define ETHTOOL_GCHANNELS	0x0000003c /* Get no of channels */
+#define ETHTOOL_SCHANNELS	0x0000003d /* Set no of channels */
+#define ETHTOOL_SET_DUMP	0x0000003e /* Set dump settings */
+#define ETHTOOL_GET_DUMP_FLAG	0x0000003f /* Get dump settings */
+#define ETHTOOL_GET_DUMP_DATA	0x00000040 /* Get dump data */
+
+/* compatibility with older code */
+#define SPARC_ETH_GSET		ETHTOOL_GSET
+#define SPARC_ETH_SSET		ETHTOOL_SSET
+
+/* Indicates what features are supported by the interface. */
+#define SUPPORTED_10baseT_Half		(1 << 0)
+#define SUPPORTED_10baseT_Full		(1 << 1)
+#define SUPPORTED_100baseT_Half		(1 << 2)
+#define SUPPORTED_100baseT_Full		(1 << 3)
+#define SUPPORTED_1000baseT_Half	(1 << 4)
+#define SUPPORTED_1000baseT_Full	(1 << 5)
+#define SUPPORTED_Autoneg		(1 << 6)
+#define SUPPORTED_TP			(1 << 7)
+#define SUPPORTED_AUI			(1 << 8)
+#define SUPPORTED_MII			(1 << 9)
+#define SUPPORTED_FIBRE			(1 << 10)
+#define SUPPORTED_BNC			(1 << 11)
+#define SUPPORTED_10000baseT_Full	(1 << 12)
+#define SUPPORTED_Pause			(1 << 13)
+#define SUPPORTED_Asym_Pause		(1 << 14)
+#define SUPPORTED_2500baseX_Full	(1 << 15)
+#define SUPPORTED_Backplane		(1 << 16)
+#define SUPPORTED_1000baseKX_Full	(1 << 17)
+#define SUPPORTED_10000baseKX4_Full	(1 << 18)
+#define SUPPORTED_10000baseKR_Full	(1 << 19)
+#define SUPPORTED_10000baseR_FEC	(1 << 20)
+#define SUPPORTED_20000baseMLD2_Full	(1 << 21)
+#define SUPPORTED_20000baseKR2_Full	(1 << 22)
+
+/* Indicates what features are advertised by the interface. */
+#define ADVERTISED_10baseT_Half		(1 << 0)
+#define ADVERTISED_10baseT_Full		(1 << 1)
+#define ADVERTISED_100baseT_Half	(1 << 2)
+#define ADVERTISED_100baseT_Full	(1 << 3)
+#define ADVERTISED_1000baseT_Half	(1 << 4)
+#define ADVERTISED_1000baseT_Full	(1 << 5)
+#define ADVERTISED_Autoneg		(1 << 6)
+#define ADVERTISED_TP			(1 << 7)
+#define ADVERTISED_AUI			(1 << 8)
+#define ADVERTISED_MII			(1 << 9)
+#define ADVERTISED_FIBRE		(1 << 10)
+#define ADVERTISED_BNC			(1 << 11)
+#define ADVERTISED_10000baseT_Full	(1 << 12)
+#define ADVERTISED_Pause		(1 << 13)
+#define ADVERTISED_Asym_Pause		(1 << 14)
+#define ADVERTISED_2500baseX_Full	(1 << 15)
+#define ADVERTISED_Backplane		(1 << 16)
+#define ADVERTISED_1000baseKX_Full	(1 << 17)
+#define ADVERTISED_10000baseKX4_Full	(1 << 18)
+#define ADVERTISED_10000baseKR_Full	(1 << 19)
+#define ADVERTISED_10000baseR_FEC	(1 << 20)
+#define ADVERTISED_20000baseMLD2_Full	(1 << 21)
+#define ADVERTISED_20000baseKR2_Full	(1 << 22)
+
+/* The following are all involved in forcing a particular link
+ * mode for the device for setting things.  When getting the
+ * devices settings, these indicate the current mode and whether
+ * it was forced up into this mode or autonegotiated.
+ */
+
+/* The forced speed, 10Mb, 100Mb, gigabit, 2.5Gb, 10GbE. */
+#define SPEED_10		10
+#define SPEED_100		100
+#define SPEED_1000		1000
+#define SPEED_2500		2500
+#define SPEED_10000		10000
+#define SPEED_UNKNOWN		-1
+
+/* Duplex, half or full. */
+#define DUPLEX_HALF		0x00
+#define DUPLEX_FULL		0x01
+#define DUPLEX_UNKNOWN		0xff
+
+/* Which connector port. */
+#define PORT_TP			0x00
+#define PORT_AUI		0x01
+#define PORT_MII		0x02
+#define PORT_FIBRE		0x03
+#define PORT_BNC		0x04
+#define PORT_DA			0x05
+#define PORT_NONE		0xef
+#define PORT_OTHER		0xff
+
+/* Which transceiver to use. */
+#define XCVR_INTERNAL		0x00
+#define XCVR_EXTERNAL		0x01
+#define XCVR_DUMMY1		0x02
+#define XCVR_DUMMY2		0x03
+#define XCVR_DUMMY3		0x04
+
+/* Enable or disable autonegotiation.  If this is set to enable,
+ * the forced link modes above are completely ignored.
+ */
+#define AUTONEG_DISABLE		0x00
+#define AUTONEG_ENABLE		0x01
+
+/* Mode MDI or MDI-X */
+#define ETH_TP_MDI_INVALID	0x00
+#define ETH_TP_MDI		0x01
+#define ETH_TP_MDI_X		0x02
+
+/* Wake-On-Lan options. */
+#define WAKE_PHY		(1 << 0)
+#define WAKE_UCAST		(1 << 1)
+#define WAKE_MCAST		(1 << 2)
+#define WAKE_BCAST		(1 << 3)
+#define WAKE_ARP		(1 << 4)
+#define WAKE_MAGIC		(1 << 5)
+#define WAKE_MAGICSECURE	(1 << 6) /* only meaningful if WAKE_MAGIC */
+
+/* L2-L4 network traffic flow types */
+#define	TCP_V4_FLOW	0x01	/* hash or spec (tcp_ip4_spec) */
+#define	UDP_V4_FLOW	0x02	/* hash or spec (udp_ip4_spec) */
+#define	SCTP_V4_FLOW	0x03	/* hash or spec (sctp_ip4_spec) */
+#define	AH_ESP_V4_FLOW	0x04	/* hash only */
+#define	TCP_V6_FLOW	0x05	/* hash only */
+#define	UDP_V6_FLOW	0x06	/* hash only */
+#define	SCTP_V6_FLOW	0x07	/* hash only */
+#define	AH_ESP_V6_FLOW	0x08	/* hash only */
+#define	AH_V4_FLOW	0x09	/* hash or spec (ah_ip4_spec) */
+#define	ESP_V4_FLOW	0x0a	/* hash or spec (esp_ip4_spec) */
+#define	AH_V6_FLOW	0x0b	/* hash only */
+#define	ESP_V6_FLOW	0x0c	/* hash only */
+#define	IP_USER_FLOW	0x0d	/* spec only (usr_ip4_spec) */
+#define	IPV4_FLOW	0x10	/* hash only */
+#define	IPV6_FLOW	0x11	/* hash only */
+#define	ETHER_FLOW	0x12	/* spec only (ether_spec) */
+/* Flag to enable additional fields in struct ethtool_rx_flow_spec */
+#define	FLOW_EXT	0x80000000
+
+/* L3-L4 network traffic flow hash options */
+#define	RXH_L2DA	(1 << 1)
+#define	RXH_VLAN	(1 << 2)
+#define	RXH_L3_PROTO	(1 << 3)
+#define	RXH_IP_SRC	(1 << 4)
+#define	RXH_IP_DST	(1 << 5)
+#define	RXH_L4_B_0_1	(1 << 6) /* src port in case of TCP/UDP/SCTP */
+#define	RXH_L4_B_2_3	(1 << 7) /* dst port in case of TCP/UDP/SCTP */
+#define	RXH_DISCARD	(1 << 31)
+
+#define	RX_CLS_FLOW_DISC	0xffffffffffffffffULL
+
+/* Reset flags */
+/* The reset() operation must clear the flags for the components which
+ * were actually reset.  On successful return, the flags indicate the
+ * components which were not reset, either because they do not exist
+ * in the hardware or because they cannot be reset independently.  The
+ * driver must never reset any components that were not requested.
+ */
+enum ethtool_reset_flags {
+	/* These flags represent components dedicated to the interface
+	 * the command is addressed to.  Shift any flag left by
+	 * ETH_RESET_SHARED_SHIFT to reset a shared component of the
+	 * same type.
+	 */
+	ETH_RESET_MGMT		= 1 << 0,	/* Management processor */
+	ETH_RESET_IRQ		= 1 << 1,	/* Interrupt requester */
+	ETH_RESET_DMA		= 1 << 2,	/* DMA engine */
+	ETH_RESET_FILTER	= 1 << 3,	/* Filtering/flow direction */
+	ETH_RESET_OFFLOAD	= 1 << 4,	/* Protocol offload */
+	ETH_RESET_MAC		= 1 << 5,	/* Media access controller */
+	ETH_RESET_PHY		= 1 << 6,	/* Transceiver/PHY */
+	ETH_RESET_RAM		= 1 << 7,	/* RAM shared between
+						 * multiple components */
+
+	ETH_RESET_DEDICATED	= 0x0000ffff,	/* All components dedicated to
+						 * this interface */
+	ETH_RESET_ALL		= 0xffffffff,	/* All components used by this
+						 * interface, even if shared */
+};
+#define ETH_RESET_SHARED_SHIFT	16
+
+#endif /* _LINUX_ETHTOOL_H */
diff --git a/include/linux/if_bonding.h b/include/linux/if_bonding.h
new file mode 100644
index 0000000..a17edda
--- /dev/null
+++ b/include/linux/if_bonding.h
@@ -0,0 +1,128 @@
+/*
+ * Bond several ethernet interfaces into a Cisco, running 'Etherchannel'.
+ *
+ *
+ * Portions are (c) Copyright 1995 Simon "Guru Aleph-Null" Janes
+ * NCM: Network and Communications Management, Inc.
+ *
+ * BUT, I'm the one who modified it for ethernet, so:
+ * (c) Copyright 1999, Thomas Davis, tadavis@lbl.gov
+ *
+ *	This software may be used and distributed according to the terms
+ *	of the GNU Public License, incorporated herein by reference.
+ *
+ * 2003/03/18 - Amir Noam <amir.noam at intel dot com>
+ *	- Added support for getting slave's speed and duplex via ethtool.
+ *	  Needed for 802.3ad and other future modes.
+ *
+ * 2003/03/18 - Tsippy Mendelson <tsippy.mendelson at intel dot com> and
+ *		Shmulik Hen <shmulik.hen at intel dot com>
+ *	- Enable support of modes that need to use the unique mac address of
+ *	  each slave.
+ *
+ * 2003/03/18 - Tsippy Mendelson <tsippy.mendelson at intel dot com> and
+ *		Amir Noam <amir.noam at intel dot com>
+ *	- Moved driver's private data types to bonding.h
+ *
+ * 2003/03/18 - Amir Noam <amir.noam at intel dot com>,
+ *		Tsippy Mendelson <tsippy.mendelson at intel dot com> and
+ *		Shmulik Hen <shmulik.hen at intel dot com>
+ *	- Added support for IEEE 802.3ad Dynamic link aggregation mode.
+ *
+ * 2003/05/01 - Amir Noam <amir.noam at intel dot com>
+ *	- Added ABI version control to restore compatibility between
+ *	  new/old ifenslave and new/old bonding.
+ *
+ * 2003/12/01 - Shmulik Hen <shmulik.hen at intel dot com>
+ *	- Code cleanup and style changes
+ *
+ * 2005/05/05 - Jason Gabler <jygabler at lbl dot gov>
+ *      - added definitions for various XOR hashing policies
+ */
+
+#ifndef _LINUX_IF_BONDING_H
+#define _LINUX_IF_BONDING_H
+
+#include <linux/if.h>
+#include <linux/types.h>
+#include <linux/if_ether.h>
+
+/* userland - kernel ABI version (2003/05/08) */
+#define BOND_ABI_VERSION 2
+
+/*
+ * We can remove these ioctl definitions in 2.5.  People should use the
+ * SIOC*** versions of them instead
+ */
+#define BOND_ENSLAVE_OLD		(SIOCDEVPRIVATE)
+#define BOND_RELEASE_OLD		(SIOCDEVPRIVATE + 1)
+#define BOND_SETHWADDR_OLD		(SIOCDEVPRIVATE + 2)
+#define BOND_SLAVE_INFO_QUERY_OLD	(SIOCDEVPRIVATE + 11)
+#define BOND_INFO_QUERY_OLD		(SIOCDEVPRIVATE + 12)
+#define BOND_CHANGE_ACTIVE_OLD		(SIOCDEVPRIVATE + 13)
+
+#define BOND_CHECK_MII_STATUS	(SIOCGMIIPHY)
+
+#define BOND_MODE_ROUNDROBIN	0
+#define BOND_MODE_ACTIVEBACKUP	1
+#define BOND_MODE_XOR		2
+#define BOND_MODE_BROADCAST	3
+#define BOND_MODE_8023AD        4
+#define BOND_MODE_TLB           5
+#define BOND_MODE_ALB		6 /* TLB + RLB (receive load balancing) */
+
+/* each slave's link has 4 states */
+#define BOND_LINK_UP    0           /* link is up and running */
+#define BOND_LINK_FAIL  1           /* link has just gone down */
+#define BOND_LINK_DOWN  2           /* link has been down for too long time */
+#define BOND_LINK_BACK  3           /* link is going back */
+
+/* each slave has several states */
+#define BOND_STATE_ACTIVE       0   /* link is active */
+#define BOND_STATE_BACKUP       1   /* link is backup */
+
+#define BOND_DEFAULT_MAX_BONDS  1   /* Default maximum number of devices to support */
+
+#define BOND_DEFAULT_TX_QUEUES 16   /* Default number of tx queues per device */
+
+#define BOND_DEFAULT_RESEND_IGMP	1 /* Default number of IGMP membership reports */
+
+/* hashing types */
+#define BOND_XMIT_POLICY_LAYER2		0 /* layer 2 (MAC only), default */
+#define BOND_XMIT_POLICY_LAYER34	1 /* layer 3+4 (IP ^ (TCP || UDP)) */
+#define BOND_XMIT_POLICY_LAYER23	2 /* layer 2+3 (IP ^ MAC) */
+
+typedef struct ifbond {
+	__s32 bond_mode;
+	__s32 num_slaves;
+	__s32 miimon;
+} ifbond;
+
+typedef struct ifslave {
+	__s32 slave_id; /* Used as an IN param to the BOND_SLAVE_INFO_QUERY ioctl */
+	char slave_name[IFNAMSIZ];
+	__s8 link;
+	__s8 state;
+	__u32  link_failure_count;
+} ifslave;
+
+struct ad_info {
+	__u16 aggregator_id;
+	__u16 ports;
+	__u16 actor_key;
+	__u16 partner_key;
+	__u8 partner_system[ETH_ALEN];
+};
+
+#endif /* _LINUX_IF_BONDING_H */
+
+/*
+ * Local variables:
+ *  version-control: t
+ *  kept-new-versions: 5
+ *  c-indent-level: 8
+ *  c-basic-offset: 8
+ *  tab-width: 8
+ * End:
+ */
+
-- 
2.5.3

