From: Chris Renshaw <osm0sis@outlook.com>
Date: Fri, 4 Dec 2015 10:52:31 -0400
Subject: [PATCH] ifplugd: add missing header

Imported from dorimanx's combined ported header toolchain:
https://github.com/dorimanx/android-busybox-ndk
---
 include/linux/mii.h | 151 ++++++++++++++++++++++++++++++++++++++++++++++++++++
 1 file changed, 151 insertions(+)
 create mode 100644 include/linux/mii.h

diff --git a/include/linux/mii.h b/include/linux/mii.h
new file mode 100644
index 0000000..def553a
--- /dev/null
+++ b/include/linux/mii.h
@@ -0,0 +1,151 @@
+/*
+ * linux/mii.h: definitions for MII-compatible transceivers
+ * Originally drivers/net/sunhme.h.
+ *
+ * Copyright (C) 1996, 1999, 2001 David S. Miller (davem@redhat.com)
+ */
+
+#ifndef __LINUX_MII_H__
+#define __LINUX_MII_H__
+
+#include <linux/types.h>
+
+/* Generic MII registers. */
+#define MII_BMCR		0x00	/* Basic mode control register */
+#define MII_BMSR		0x01	/* Basic mode status register  */
+#define MII_PHYSID1		0x02	/* PHYS ID 1                   */
+#define MII_PHYSID2		0x03	/* PHYS ID 2                   */
+#define MII_ADVERTISE		0x04	/* Advertisement control reg   */
+#define MII_LPA			0x05	/* Link partner ability reg    */
+#define MII_EXPANSION		0x06	/* Expansion register          */
+#define MII_CTRL1000		0x09	/* 1000BASE-T control          */
+#define MII_STAT1000		0x0a	/* 1000BASE-T status           */
+#define MII_ESTATUS		0x0f	/* Extended Status             */
+#define MII_DCOUNTER		0x12	/* Disconnect counter          */
+#define MII_FCSCOUNTER		0x13	/* False carrier counter       */
+#define MII_NWAYTEST		0x14	/* N-way auto-neg test reg     */
+#define MII_RERRCOUNTER		0x15	/* Receive error counter       */
+#define MII_SREVISION		0x16	/* Silicon revision            */
+#define MII_RESV1		0x17	/* Reserved...                 */
+#define MII_LBRERROR		0x18	/* Lpback, rx, bypass error    */
+#define MII_PHYADDR		0x19	/* PHY address                 */
+#define MII_RESV2		0x1a	/* Reserved...                 */
+#define MII_TPISTATUS		0x1b	/* TPI status for 10mbps       */
+#define MII_NCONFIG		0x1c	/* Network interface config    */
+
+/* Basic mode control register. */
+#define BMCR_RESV		0x003f	/* Unused...                   */
+#define BMCR_SPEED1000		0x0040	/* MSB of Speed (1000)         */
+#define BMCR_CTST		0x0080	/* Collision test              */
+#define BMCR_FULLDPLX		0x0100	/* Full duplex                 */
+#define BMCR_ANRESTART		0x0200	/* Auto negotiation restart    */
+#define BMCR_ISOLATE		0x0400	/* Isolate data paths from MII */
+#define BMCR_PDOWN		0x0800	/* Enable low power state      */
+#define BMCR_ANENABLE		0x1000	/* Enable auto negotiation     */
+#define BMCR_SPEED100		0x2000	/* Select 100Mbps              */
+#define BMCR_LOOPBACK		0x4000	/* TXD loopback bits           */
+#define BMCR_RESET		0x8000	/* Reset to default state      */
+
+/* Basic mode status register. */
+#define BMSR_ERCAP		0x0001	/* Ext-reg capability          */
+#define BMSR_JCD		0x0002	/* Jabber detected             */
+#define BMSR_LSTATUS		0x0004	/* Link status                 */
+#define BMSR_ANEGCAPABLE	0x0008	/* Able to do auto-negotiation */
+#define BMSR_RFAULT		0x0010	/* Remote fault detected       */
+#define BMSR_ANEGCOMPLETE	0x0020	/* Auto-negotiation complete   */
+#define BMSR_RESV		0x00c0	/* Unused...                   */
+#define BMSR_ESTATEN		0x0100	/* Extended Status in R15      */
+#define BMSR_100HALF2		0x0200	/* Can do 100BASE-T2 HDX       */
+#define BMSR_100FULL2		0x0400	/* Can do 100BASE-T2 FDX       */
+#define BMSR_10HALF		0x0800	/* Can do 10mbps, half-duplex  */
+#define BMSR_10FULL		0x1000	/* Can do 10mbps, full-duplex  */
+#define BMSR_100HALF		0x2000	/* Can do 100mbps, half-duplex */
+#define BMSR_100FULL		0x4000	/* Can do 100mbps, full-duplex */
+#define BMSR_100BASE4		0x8000	/* Can do 100mbps, 4k packets  */
+
+/* Advertisement control register. */
+#define ADVERTISE_SLCT		0x001f	/* Selector bits               */
+#define ADVERTISE_CSMA		0x0001	/* Only selector supported     */
+#define ADVERTISE_10HALF	0x0020	/* Try for 10mbps half-duplex  */
+#define ADVERTISE_1000XFULL	0x0020	/* Try for 1000BASE-X full-duplex */
+#define ADVERTISE_10FULL	0x0040	/* Try for 10mbps full-duplex  */
+#define ADVERTISE_1000XHALF	0x0040	/* Try for 1000BASE-X half-duplex */
+#define ADVERTISE_100HALF	0x0080	/* Try for 100mbps half-duplex */
+#define ADVERTISE_1000XPAUSE	0x0080	/* Try for 1000BASE-X pause    */
+#define ADVERTISE_100FULL	0x0100	/* Try for 100mbps full-duplex */
+#define ADVERTISE_1000XPSE_ASYM	0x0100	/* Try for 1000BASE-X asym pause */
+#define ADVERTISE_100BASE4	0x0200	/* Try for 100mbps 4k packets  */
+#define ADVERTISE_PAUSE_CAP	0x0400	/* Try for pause               */
+#define ADVERTISE_PAUSE_ASYM	0x0800	/* Try for asymetric pause     */
+#define ADVERTISE_RESV		0x1000	/* Unused...                   */
+#define ADVERTISE_RFAULT	0x2000	/* Say we can detect faults    */
+#define ADVERTISE_LPACK		0x4000	/* Ack link partners response  */
+#define ADVERTISE_NPAGE		0x8000	/* Next page bit               */
+
+#define ADVERTISE_FULL		(ADVERTISE_100FULL | ADVERTISE_10FULL | \
+				  ADVERTISE_CSMA)
+#define ADVERTISE_ALL		(ADVERTISE_10HALF | ADVERTISE_10FULL | \
+				  ADVERTISE_100HALF | ADVERTISE_100FULL)
+
+/* Link partner ability register. */
+#define LPA_SLCT		0x001f	/* Same as advertise selector  */
+#define LPA_10HALF		0x0020	/* Can do 10mbps half-duplex   */
+#define LPA_1000XFULL		0x0020	/* Can do 1000BASE-X full-duplex */
+#define LPA_10FULL		0x0040	/* Can do 10mbps full-duplex   */
+#define LPA_1000XHALF		0x0040	/* Can do 1000BASE-X half-duplex */
+#define LPA_100HALF		0x0080	/* Can do 100mbps half-duplex  */
+#define LPA_1000XPAUSE		0x0080	/* Can do 1000BASE-X pause     */
+#define LPA_100FULL		0x0100	/* Can do 100mbps full-duplex  */
+#define LPA_1000XPAUSE_ASYM	0x0100	/* Can do 1000BASE-X pause asym*/
+#define LPA_100BASE4		0x0200	/* Can do 100mbps 4k packets   */
+#define LPA_PAUSE_CAP		0x0400	/* Can pause                   */
+#define LPA_PAUSE_ASYM		0x0800	/* Can pause asymetrically     */
+#define LPA_RESV		0x1000	/* Unused...                   */
+#define LPA_RFAULT		0x2000	/* Link partner faulted        */
+#define LPA_LPACK		0x4000	/* Link partner acked us       */
+#define LPA_NPAGE		0x8000	/* Next page bit               */
+
+#define LPA_DUPLEX		(LPA_10FULL | LPA_100FULL)
+#define LPA_100			(LPA_100FULL | LPA_100HALF | LPA_100BASE4)
+
+/* Expansion register for auto-negotiation. */
+#define EXPANSION_NWAY		0x0001	/* Can do N-way auto-nego      */
+#define EXPANSION_LCWP		0x0002	/* Got new RX page code word   */
+#define EXPANSION_ENABLENPAGE	0x0004	/* This enables npage words    */
+#define EXPANSION_NPCAPABLE	0x0008	/* Link partner supports npage */
+#define EXPANSION_MFAULTS	0x0010	/* Multiple faults detected    */
+#define EXPANSION_RESV		0xffe0	/* Unused...                   */
+
+#define ESTATUS_1000_TFULL	0x2000	/* Can do 1000BT Full          */
+#define ESTATUS_1000_THALF	0x1000	/* Can do 1000BT Half          */
+
+/* N-way test register. */
+#define NWAYTEST_RESV1		0x00ff	/* Unused...                   */
+#define NWAYTEST_LOOPBACK	0x0100	/* Enable loopback for N-way   */
+#define NWAYTEST_RESV2		0xfe00	/* Unused...                   */
+
+/* 1000BASE-T Control register */
+#define ADVERTISE_1000FULL	0x0200  /* Advertise 1000BASE-T full duplex */
+#define ADVERTISE_1000HALF	0x0100  /* Advertise 1000BASE-T half duplex */
+#define CTL1000_AS_MASTER	0x0800
+#define CTL1000_ENABLE_MASTER	0x1000
+
+/* 1000BASE-T Status register */
+#define LPA_1000LOCALRXOK	0x2000	/* Link partner local receiver status */
+#define LPA_1000REMRXOK		0x1000	/* Link partner remote receiver status */
+#define LPA_1000FULL		0x0800	/* Link partner 1000BASE-T full duplex */
+#define LPA_1000HALF		0x0400	/* Link partner 1000BASE-T half duplex */
+
+/* Flow control flags */
+#define FLOW_CTRL_TX		0x01
+#define FLOW_CTRL_RX		0x02
+
+/* This structure is used in all SIOCxMIIxxx ioctl calls */
+struct mii_ioctl_data {
+	__u16		phy_id;
+	__u16		reg_num;
+	__u16		val_in;
+	__u16		val_out;
+};
+
+#endif /* __LINUX_MII_H__ */
-- 
2.5.3

